V410H

Intelligent Operation and Efficient Flight
The V410H is a high efficiency, multi-purpose composite fixed wings and Drone hybrid product with a VTOL fuselage portable design. Made of carbon fiber layers. Disassembly, assembly and small footprint.
It is a fixed-wing Cloud Sub-Autonomous Aircraft that can take off and land vertically. In horizontal cruising, there is a system powered by a gasoline engine, and in vertical take-off and landing, there is support from electric motors, thus creating a platform with a longer flight time.
 
Autonomous Mission Capability
Runway-independent, vertical take-off
Day and night, execution, surveillance and intelligence
shot arrangement
From the management of the UAV from the Single Ground Control Station
Subcloud task execution
Autonomous Flight System
Unique autopilot system
Return home and auto landing in case of disconnection
Unique Ground Control station system
 
General Mission Capabilities
Residential Thermal Measurement
Forest Fire Management
Post Disaster Assessment
Bilge and Environmental Pollution Detection
Agricultural Applications
Cartography
Tracking, Detection and Area Protection
Intelligence
Electronic Harp
Coastal and Border Security
Energy Transmission and Oil-Gas Lines Inspection
Anti-Smuggling and Anti-Terrorism
Public order
Narcotic Plant Detection

Mechanical and Flight Parameters
Dimensions 4100x2215x786mm
Communication Distance 30 km
(optional 150km)
Flight Time 600 min. (with Payload)
Maximum flight altitude 5000 m (MSL)
Maximum Travel Speed 104 km/h
Stall Speed 61 km/h
Maximum Wind Limit (VTOL) 10 m/s
Maximum Wind Time (Fixed Wing) 17 m/s
Operational Range 200km